Open topic with navigation

# IndexPort

The port number to use to send index actions to HPE Content Component.

Type: | Long
Default: | 9001
Allowed Range: | Minimum: 1 Maximum: 65535
Recommended Range: | Minimum: 1025 Maximum: 65535
Required: | No
Configuration Section: | Server
Example: | `IndexPort=59001`
See Also: | IndexClients Port

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm