Open topic with navigation

# ExpireTime

The time to run the first DREEXPIRE operation. Specify the time in the 24-hour clock, in the format `hh:mm`.

When you start HPE Content Component, the specified ExpireInterval must elapse (after the specified `ExpireTime`) before the first DREEXPIRE takes place.

Type: | String
Default: |
Required: | Yes, if you have set `Expire` to `True`
Configuration Section: | Schedule
Example: |
    ExpireInterval=12:00
    ExpireTime=19:00
In this example, if you start HPE Content Component at 18:00, the first expiry operation occurs at 07:00 the following day.
See Also: | Expire ExpireInterval

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm