Open topic with navigation

# TermCachePersistentKB

The amount of memory to allocate to store the most commonly occurring terms.

If you set `TermCachePersistentKB`, the `N` most commonly occurring terms (by total number of occurrences) are stored in memory. `N` is selected so that the amount of memory used to store the terms is as close as possible to the memory allocated in `TermCachePersistentKB`. The default value is `0` (zero), which means that HPE Content Component does not cache terms.

Use this parameter only when there is a large amount of available memory, such as in 64-bit applications.

If you set both TermCachePersistentMinOccs and `TermCachePersistentKB`, `TermCachePersistentKB` takes precedence.

Type: | Long
Default: | 0
Allowed Range: | Minimum: 0 Maximum: N/A
Recommended Range: | Minimum: 10240 Maximum: 2048000
Required: | No
Configuration Section: | TermCache
Example: | `TermCachePersistentKB=100000`
See Also: | TermCachePersistentMinOccs

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm