Open topic with navigation

# ExpireTime

The number of seconds after which the flush lock must expire, in case the HPE Content Component that holds the lock becomes unavailable.

Type: | Long
Default: | 1000
Required: | No
Configuration Section: | MyLockServer
Example: | `ExpireTime=3600`
See Also: |

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm