# Color Clustering

Color clustering determines the dominant colors in an image or video frame by clustering similar colors. The task returns the color at the center of each cluster, and the proportion of the pixels that belong to each cluster. If you configure a color dictionary, the task clusters colors around the colors that are defined in the dictionary, and returns a name (such as "light blue" or "red") for each cluster.

Configuration Parameter | Description
--- | ---
ColorDictionary | A dictionary file that associates names with RGB color values.
ColorSpace | The color space in which the results of analysis are provided.
ColorThreshold | Any color cluster with a score that does not meet the specified threshold is omitted from the results.
CombineNamedColors | A Boolean value that specifies whether to combine clusters that have the same color name.
Input | The image track to process.
MaxInputQueueLength | Can be used to place a limit on latency.
NumParallel | The maximum number of video frames to analyze simultaneously.
Region | Specifies a region of the frame to process, instead of the entire frame.
RegionUnit | (Deprecated) Specifies the units used by the `Region` parameter.
RestrictToInputRegion | (Deprecated) Specifies whether to analyze a region of the input image or video frame that is specified in the input record, instead of the entire image.
SampleInterval | The interval at which frames are selected to be analyzed.
SegmentDuration | The maximum duration of a record in the `SegmentedResult` track.
Type | The analysis engine to use. Set this parameter to `ColorCluster`.

## Output Tracks

Output track | Description | Output1This column indicates whether the information contained in the track is included by default in the output created by an output task (when you don't set the Input parameter for the output task).
--- | --- | ---
`Data` | Contains one record, describing the analysis results, for each input record. | No
`Result` | Contains a record, describing the analysis results, for each event. When the input is images, Media Server considers each image separately. When the input is video from an ingest engine, or an engine that does not support tracking, Media Server begins a new result when there is a significant change in the color clustering. When the input is video from an engine that supports tracking (for example number plate recognition), results begin and end at the times provided by the other analysis task (for example when the vehicle appears and disappears). The IDs used for the color cluster records are also inherited from the input records. | Yes
`SegmentedResult` | (Available only when processing video). The same as the `Result` track, except the duration of each record is limited by the parameter SegmentDuration. If a result exceeds the specified duration, Media Server begins a new record with the same ID. | Yes
`Start` | The same as the `Data` track, except it contains only the first record of each event. | No
`End` | The same as the `Data` track, except it contains only the last record of each event. | No
`ClusteredImage` | Contains one record for each event. Each record contains the source image, cropped to the analyzed region and modified so that it only contains colors that match the center of a color cluster. If the analyzed region is not rectangular any pixels outside the region are transparent (or black if you use an image format that does not support transparency). | No

_FT_HTML5_bannerTitle.htm