Distributed Action Handler 24.1

# DAHEngine`N` Configuration

In the `[DAHEngines]` section you must create a `[DAHEngineN]` subsection for each IDOL server to which the Distributed Action Handler sends actions. Each `[DAHEngineN]` subsection specifies the host and ACI port of a child IDOL server. See Child Server Configuration Parameters.

NOTE: You must number child IDOL server sections in consecutive order, starting from 0 (zero).

For example:

    [DAHEngines]
    Number=2

    [DAHEngine0]
    Host=localhost
    Port=9000

    [DAHEngine1]
    Host=12.3.4.56
    Port=9000

Copyright 2023 Open Text
Version 24.1 | Last updated December 2023

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: IDOL Distributed Action Handler 24.1

Topic Title: DAHEngineN Configuration