# RecorderPort

The TCP port of the XProtect recording server. Media Server receives video from the recording server.

Type: | Integer
Default: | If SOAPAuthentication is set to `false`, or the engine detects that it has logged on to an XProtect Enterprise system, the default value is `80`. If SOAPAuthentication is set to `true` and the engine detects that it has logged on to an XProtect Corporate system, the default value is `7563`.
Required: | No
Configuration Section: | TaskName
Example: | `RecorderPort=7563`
See Also: | RecorderHost

_FT_HTML5_bannerTitle.htm